Hamlet

Running List

Pre- Show Checks

* Turn on Glaciator at 13Amp socket, the power switch on the Glaciator, and insert the PVC pipe
* Ensure a mat is placed infront of the Glaciator PVC pipe on stage to prevent slips, trips and falls
* Close the door with the magnetic catch
* Check the Patt 23’s are plugged in
* Check TSM ropes for signs of wear as lanterns are close by

Post-Show Checks

* Ensure stage is clear of cables
* Turn Glaciator off at the 13Amp socket and remove PVC pipe