Power up/Power down procedure – Sound on WWoD

Power up:

1. Power up the control room stage box, the desk CPU (both located in the Ath control room).
2. Power on the channel receivers and the sound world in the SL void.
3. Power on the desk and load up the show file.
4. Connect the **powered** **down** laptop to the FireWire/thunderbolt cable for the Focusrite Saffire.
5. Power on the Focusrite interface and the laptop and check to make sure the two green LEDs on the interface are live – this indicates that there is power to the interface and that the FireWire connection is active.
6. Once the control system is active, the speaker amplifiers can be safely turned on. There is an amplifier rack in the control room that must all be power on. There is a stage amplifier that controls the two MAX monitors under the rake (the amp is located mid void). The last amplifier is located in the auditorium left side God’s platform.

Power down:

1. The amplifiers need to be powered off before anything else.
2. After the amplifiers have all been powered off, the computer and Focusrite system can be powered off safely.
3. Before the desk is powered down, save your show and back it up to a flash drive.
4. The desk can then be powered down.
5. The stage box, control room stage box and desk CPU, as well as the radio channel receivers can be powered down.