Boom

How it was built: scaff pole of a height of 3000mm with boom arms with ETC source 4 LED 26deg at a height of 2500mm, ETC CE source 4 19deg at a 2000mm, 2 ETC source4 Fresnel at heights of 1250mm and 900mm and finally selecon arena high performance Fresnel at a height of 300mm. The boom is on a dolly which also has stage weights on the base plates to make sure that there is no chance of the boom falling over. There is a tab track size of 2240mm by 630mm that allows the boom to move back allowing the flying/changes to happen, for monkey and snake.

