Sunday in the Park with George

**LX Department – Power Up/ Down Procedure**

|  |
| --- |
| **Power Up** |
|  | Get isolation from client services (red form – haze, smoke and grid) |
|  | Turn on workers at DSL trip board |
|  | Turn on stage power, stage basement power, SR and SL fly floor, auditorium roof at DSL trip board |
|  | Turn on independent 4 at DSL trip board |
|  | Turn on 32a breaker wheel (top) in auditorium gods |
|  | Turn on 1st circle power at switch in Ath control room – Power on projector |
|  | Power up hazer on SL flys (ensure isolation is in place!) |

|  |
| --- |
| **Power Down** |
|  | Turn off hazer and unplug at source on SL flys |
|  | Turn off projector – Turn off 1st circle power at switch in Ath control room |
|  | Turn off 32a breaker wheel (top) in auditorium gods |
|  | Turn off independent 4 at DSL trip board |
|  | Turn off stage power, stage basement power, SR and SL fly floor, auditorium roof at DSL trip board |
|  | Turn off workers at DSL trip board |